> - Downloads
> - Configuring the Pseudo-RADIUS Server for External Subscriber Monitor
> - Related Topics
> - Configuring the Pseudo-RADIUS Server for External Subscriber Monitor (C-Web Interface)
> - Configuring External Subscriber Monitor
> - Configuring Event Notification for External Subscriber Monitor
> - Configuring the NIC Proxy for the Pseudo-RADIUS Server
> - Viewing Statistics for External Subscriber Monitor

> # Configuring the Pseudo-RADIUS Server for External Subscriber Monitor

> Use the following configuration statements to configure External Subscriber Monitor as a RADIUS accounting server:

> `
> slot number external-subscriber-monitor radius-accounting {
>   port port;
>   service-type (all | login | framed | callback-login | callback-framed | outbound | administrative | nas-prompt | authenticate-only | callback-nas-prompt | callback-check | callback-administrative);
>   allow [allow...];
>   deny [deny...];
>   maximum-queue-length maximum-queue-length;
> }
> `

> To configure the RADIUS accounting server:

> 1. From configuration mode, access the configuration statement that configures the RADIUS server.
>    `
>    user@host# edit slot 0 external-subscriber-monitor radius-accounting
>    `
> 2. (Optional) Specify the listening port for RADIUS requests.
>    `
>    [edit slot 0 external-subscriber-monitor radius-accounting]
>    user@host# set port port
>    `
> 3. (Optional) Specify the service type of the RADIUS packets that will be forwarded.
>    `
>    [edit slot 0 external-subscriber-monitor radius-accounting]
>    user@host# set service-type service-type
>    `
> 4. (Optional) Specify a list that filters which packets are forwarded to the SAE based on NAS ID or NAS IP.
>    `
>    [edit slot 0 external-subscriber-monitor radius-accounting]
>    user@host# set allow [allow...]
>    `
> 5. (Optional) Specify a list that filters which packets are forwarded to the SAE based on NAS ID or NAS IP.
>    `
>    [edit slot 0 external-subscriber-monitor radius-accounting]
>    user@host# set deny [deny... ]
>    `
> 6. Specify the maximum number of unacknowledged RADIUS messages to be received from the RADIUS server before it discards new messages.
>    `
>    [edit slot 0 external-subscriber-monitor radius-accounting]
>    user@host# set maximum-queue-length set maximum-queue-length
>    `
> 7. (Optional) Verify your configuration.
>    `
>    [edit slot 0 external-subscriber-monitor radius-accounting]
>    user@host# show
>    `

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.