> - Downloads
> - Configuring an SAE Group
> - Related Topics
> - Configuring an SAE Group with the C-Web Interface
> - Creating Grouped Configurations for the SAE (SRC CLI)
> - Initially Configuring the SAE
> - Deleting Default Configurations Within an SAE Group
> - Configuring Local Properties for the SAE (SRC CLI)

> # Configuring an SAE Group

> Use the shared option of the set slot number sae shared command to add a new group. Use the shared sae group name command to configure the group.

> To configure a group:

> 1. From configuration mode, add a group. For example, to add a group called REGION-1 in the path /SAE/:
>    `
>    [edit]
>    user@host# set slot 0 sae shared /SAE/REGION-1
>    `
> 2. Commit the configuration.
>    `
>    [edit]
>    user@host# commit
>    commit complete.
>    `
> 3. Configure the group as you would a shared SAE configuration.

>        [edit]
>        user@host# edit shared sae group REGION-1 ?
>        Possible completions:
>          <[Enter]>           Execute this command
>        > configuration
>        > dhcp-classifier Configure a DHCP classification script
>        > group               Group of SAE configuration properties
>        > user-classifier Configure a subscriber classification script
>          |                    Pipe through a command

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.