[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the SAE to Manage JUNOSe Routers (C-Web Interface)

To set up the SAE to manage JUNOSe routers, configure a router driver that specifies a COPS server that can accept COPS connections from the COPS client in JUNOSe routers.

To configure the SAE to manage JUNOSe routers:

1. Click Configure, expand Shared>SAE>Configuration>Driver, and then click JUNOSe.

   The JUNOSe pane appears.

2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

#### Related Topics

- Configuring the SAE to Manage JUNOSe Routers with the CLI
- Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices
- Monitoring Interactions Between the SAE and the JUNOSe Router
- Troubleshooting Problems with Managing JUNOSe Routers
- COPS Connection Between JUNOSe Routers and the SAE

[Contents] [Prev] [Next] [Index] [Report an Error]