[Contents] [Prev] [Next] [Index] [Report an Error]

# Specifying Router Initialization Scripts on the SAE

Use the following configuration statements to specify router initialization scripts for JUNOS routing platforms:

`

shared sae configuration driver scripts {
  extension-path extension-path ;
  general general ;
  junos junos ;
}

`

To configure router initialization scripts for JUNOS routing platforms:

1. From configuration mode, access the configuration statements that configure router initialization scripts. In this sample procedure, the scripts are configured in the west-region group.
   `
   user@host# edit shared sae group west-region configuration driver scripts
   `
2. Specify the router initialization script for JUNOS routing platforms.
   `
   [edit shared sae group west-region configuration driver scripts]
   user@host# set junos junos
   `
3. Configure a router initialization script that can be used for all types of routers that the SRC module supports.
   `
   [edit shared sae group west-region configuration driver scripts]
   user@host# set general general
   `
4. Configure a path to router initialization scripts that are not in the default location, /opt/UMC/sae/lib.
   `
   [edit shared sae group west-region configuration driver scripts]
   user@host# set extension-path extension-path
   `
5. (Optional) From operational mode, verify your router initialization script configuration.

       [edit shared sae group west-region configuration driver scripts]
       user@host# show
       extension-path ;
       junos iorPublisher;

#### Related Topics

- Specifying JUNOS Router Initialization Scripts on the SAE (C-Web Interface)
- Configuring JUNOS Routing Platforms to Interact with the SAE
- Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices

[Contents] [Prev] [Next] [Index] [Report an Error]