[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Statistics for Device Drivers with the CLI

#### Purpose

View SNMP statistics for all device drivers.

#### Action

`user@host> show sae statistics device common`

    SNMP Statistics
    Driver type                    JUNOSE COPS
    Number of close requests       0
    Number of connections accepted 0
    Number of current connections  0
    Number of open requests        0
    Server address                 0.0.0.0
    Server port                    3288
    Time since last redirect       0

    SNMP Statistics
    Driver type                    PACKETCABLE COPS
    Number of close requests       0
    Number of connections accepted 0
    Number of current connections  0
    Number of open requests        0
    Server address                 0.0.0.0
    Server port                    0
    Time since last redirect       0

    SNMP Statistics
    Driver type                    JUNOS
    Number of close requests       0
    Number of connections accepted 0
    Number of current connections  0
    Number of open requests        0
    Server address                 0.0.0.0
    Server port                    3333
    Time since last redirect       0

The value of the server address can be either an IPv4 or IPv6 address, depending on the platform.

#### Related Topics

- Shutting Down the Device Drivers (C-Web Interface)
- Viewing Information About SAE Device Drivers with the CLI
- Viewing SNMP Information for Routers and Devices with the CLI
- Viewing Statistics for Specific Device Drivers with the CLI

[Contents] [Prev] [Next] [Index] [Report an Error]