[Contents] [Prev] [Next] [Index] [Report an Error]

# Setting Up MX Series Routers in the SRC Network (SRC CLI)

To set up the MX Series router so that the router can be managed by the SAE:

1. From configuration mode, access the configuration statement that configures network devices. This sample procedure uses mx_device as the name of the router.
   `
   user@host# edit slot 0 shared network device mx_device
   `
2. Set the type of device to third-party.
   `
   [edit shared network device mx_device]
   user@host# set device-type third-party
   `
3. From configuration mode, access the configuration statements for virtual routers. For MX Series routers, use the name default for the virtual router.
   `
   [edit shared network device mx_device]
   user@host# edit virtual-router default
   `
4. Specify the addresses of SAEs that can manage this router.
   `
   [edit shared network device mx_device virtual-router default]
   user@host# set sae-connection [sae-connection...]
   `

[Contents] [Prev] [Next] [Index] [Report an Error]