> - Downloads
> - Specifying Port Access for Traffic Classification (SRC CLI)
> - Related Topics
> - Before You Configure Classify-Traffic Conditions
> - Configuring Classify-Traffic Conditions
> - Enabling Expansion of JUNOSe Classify-Traffic Conditions (SRC CLI)
> - Specifying the PCMM Classifier Type (SRC CLI)
> - Specifying Port Access for Traffic Classification (C-Web Interface)

> # Specifying Port Access for Traffic Classification (SRC CLI)

> In the SRC software, the way that you specify a range of port numbers greater than or less than a specific value in a traffic classifier is different from the way you define a range in the configuration on routers running JUNOSe Software.

> In the SRC CLI, you specify ranges by setting values in the port-operation options in command statements.

> To specify a range of port numbers greater or less than a specified value, you can:

> - Define the full set of port numbers in the range to be allowed.
> - Define the full set of port numbers in the range not allowed.

> To configure port numbers greater than a defined value by specifying which values are allowed:

> 1. For the port-operation option, enter eq.
> 2. For the from-port option, enter the range of ports allowed.

>    For example, to specify access to all port numbers greater than 10, specify 11..65535.

> To configure port numbers greater than a defined value by specifying which values are not allowed:

> 1. For the port-operation option, enter neq.
> 2. For the from-port option, enter the range of ports not allowed.

>    For example, to specify access to all port numbers greater than 10, specify 1..9.

> To configure port numbers less than a defined value by specifying which values are allowed:

> 1. For the port-operation option, enter eq.
> 2. For the from-port option, enter the range of ports.

>    For example, to specify access to all port numbers less than 10, specify 1..9.

> To configure port numbers less than a defined value by specifying which values are not allowed:

> 1. For the port-operation option, enter neq.
> 2. For the from-port option, enter the range of ports.

>    For example, to specify access to all port numbers less than 10, specify 11..65535.

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.