[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Power Status of a Controller Using IPMI

You can view IPMI power information for the controller you are currently logged on to and for a remote controller. You must be logged in as a root user.

To display power status (on or off) of the local controller using IPMI:

1. Log in as root user.
   `
   SRC-PE Release 3.1 [R.3.1.0-12]
   login: root
   `
2. Enter the password.
   `
   Password: password
   `

   You are now logged in as root user.

3. Access the CLI.
   `
   [root@host ~]# cli
   --- SRC CLI 3.1 build CLI.R.3.1.0.012
   (c) 2005-2008 Juniper Networks Inc.
   root@host>
   `
4. Enter the show ipmi power command.

   For example:

   `root@host>show ipmi power`

       Chassis Power is on

To display power status information on a remote controller using IPMI:

1. Log in as root user.
2. Enter the show ipmi host power command.
   `
   root@host>show ipmi host host user user power
   `
   - host—IP address of remote host IPMI interface
   - user—IPMI username configured in the remote host

   For example:

   `
   root@host>show ipmi host 10.10.10.30 user johndoe power
   `

[Contents] [Prev] [Next] [Index] [Report an Error]