> - Downloads
> - Configuring Subscriber IP Pools as IP Subnets
> - Related Topics
> - Configuring Subscriber IP Pools as IP Subnets (C-Web Interface)
> - Modifying the Subscriber Configuration
> - Configuring Subscriber IP Pools as IP Address Ranges
> - Specifying Connections to CMTS Devices

> # Configuring Subscriber IP Pools as IP Subnets

> To configure subscriber IP pools that are managed by the CMTS device as IP subnets:

> 1. From configuration mode, access the configuration statement that configures the CMTS device to which the JPS can connect.
>    `
>    user@host# edit slot 0 jps cmts-registry cmts cmts-ip subnet-pool subnet
>    `

>    Specify the IP address of the CMTS device and the IP address and mask of the subnet for the pool of subscriber IP addresses.

> 2. (Optional) Specify the IP addresses of the subnet that are excluded from the subscriber IP pool managed by the CMTS device.
>    `
>    [edit slot 0 jps cmts-registry cmts cmts-ip subnet-pool subnet]
>    user@host# set exclude [exclude...]
>    `
> 3. (Optional) Verify your configuration.

>        [edit slot 0 jps cmts-registry]
>        user@host# show

> #### Published: 2009-09-23

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.