[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Initial Directory Eventing Properties for IMS (SRC CLI)

Use the following configuration statements to configure directory eventing properties for IMS:

`

slot number ims initial directory-eventing {
  eventing;
  signature-dn signature-dn;
  polling-interval polling-interval;
  event-base-dn event-base-dn;
  dispatcher-pool-size dispatcher-pool-size;
}

`

To configure initial directory eventing properties:

1. From configuration mode, access the statement that configures the local properties.
   `
   user@host# edit slot 0 ims initial eventing
   `
2. Specify the initial directory eventing properties for IMS.
   `
   [edit slot 0 ims initial directory-eventing]
   user@host# set ?
   `

   For more information about configuring local properties for the SRC components, see Configuring Basic Local Properties.

3. (Optional) Verify your configuration.

       [edit slot 0 ims initial directory-eventing]
       user@host# show
       eventing;
       polling-interval 30;

#### Related Topics

- Overview of an IMS Environment
- Configuring the IMS Software (SRC CLI)
- Configuring Initial Properties for IMS (SRC CLI)
- Configuring Directory Connection Properties for IMS (SRC CLI)
- Configuration Statements for IMS Support

[Contents] [Prev] [Next] [Index] [Report an Error]