> - Downloads
> - Viewing Information About SAE Device Drivers with the CLI
> - Related Topics
> - Initially Configuring the SAE
> - Shutting Down the Device Drivers
> - Viewing Information About Device Drivers
> - Viewing Statistics for Device Drivers with the CLI

> # Viewing Information About SAE Device Drivers with the CLI

> #### Purpose

> View information about SAE device drivers. Each device driver manages one logical router instance.

> #### Action

> To view information about the state of SAE device drivers:

> `user@host> show sae drivers`

>     JUNOSe Driver
>     Device name                           default@dryad
>     Device type                           junose
>     Device IP                             10.227.7.244
>     Local IP                              10.227.7.172
>     TransportRouter                       default@dryad
>     Device version                        7.2.0
>     Start time                            Tue Feb 13 14:18:44 EST 2007
>     Number of notifications               20
>     Number of processed added             14
>     Number of processed changed           0
>     Number of processed deleted           6
>     Number of provisioning attempt        30
>     Number of provisioning attempt failed 0
>     Number of outstanding decisions       0
>     Number of SAP                         7
>     Number of PAP                         1
>       Job Queue
>       Size                  0
>       Age (ms)              1
>       Total enqueued        28
>       Total dequeued        28
>       Average job time (ms) 426
>       State Synchronization
>       Number recovered subscriber sessions              0
>       Number recovered service sessions                 0
>       Number recovered interface sessions               0
>       Number invalid subscriber sessions                0
>       Number invalid service sessions                   0
>       Number invalid interface sessions                 0
>       Background restoration start time                 Tue Feb 13 14:18:49 EST 2007
>       Background restoration end time                   Tue Feb 13 14:18:49 EST 2007
>       Number subscriber sessions restored in background 0
>       Number of provisioning objects left to collect    0
>       Total number of provisioning objects to collect   11
>       Start time                                        Tue Feb 13 14:18:45 EST 2007
>       End time                                          Tue Feb 13 14:18:47 EST 2007
>       Number of synched contexts                        7
>       Number of post-sync jobs                          6

> To view information about the state of a particular device driver, specify all or part of the virtual router name. For JUNOS router drivers and PCMM drivers, use the format default@routerName.

> `user@host> show sae drivers device-name device-name`
> `
> `

> To view only the virtual router names for the device driver:

> `user@host> show sae drivers brief`

>     Router Drivers
>     Router Name              Router Type
>     default@simJunos            junos

> To restrict the number of displayed results:

> `user@host> show sae drivers maximum-results maximum-results`
> `
> `

> #### Published: 2009-09-10

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.