> - Downloads
> - Setting Up SAE Communities (SRC CLI)
> - Related Topics
> - Using the SAE in a PCMM Environment
> - Setting Up SAE Communities (C-Web Interface)
> - Initially Configuring the SAE
> - Configuring SAE Properties for the Event Notification API (SRC CLI)

> # Setting Up SAE Communities (SRC CLI)

> You can configure the following for SAE communities:

> - Define the members of an SAE community by adding the IP addresses of SAEs in the community to the virtual router object of the network device in the directory.

>   See Creating Virtual Routers for the CMTS Device (SRC CLI) .

> - Configure parameters for the SAE community manager.

>   See Configuring the SAE Community Manager .

> - Specify the name of the community manager with the set sae-community-manager option in the PCMM driver configuration.

>   See Configuring the SAE to Manage PCMM Devices (SRC CLI).

> - If there is a firewall in the network, configure the firewall to allow SAE messages through.

> #### Published: 2009-09-23

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.