> - Downloads
> - Initially Configuring the SAE with the C-Web Interface
> - Related Topics
> - Initially Configuring the SAE
> - Starting the SAE with the C-Web Interface
> - Configuring LDAP Access to Directory Data with the C-Web Interface
> - Reloading the SAE Configuration
> - Configuring the SAE to Store Log Messages in a File (C-Web Interface)

> # Initially Configuring the SAE with the C-Web Interface

> To initially configure the SAE:

> - (Optional) Create a configuration group for the SAE.

>   See Configuring an SAE Group with the C-Web Interface

> - Configure local properties for the SAE.

>   See Configuring Local Properties for the SAE with the C-Web Interface

> - Configure a local IP address and NAS ID that the SAE uses to communicate with RADIUS servers.

>   See Configuring the RADIUS Local IP Address and NAS ID with the C-Web Interface

> - Configure the location of the directory that contains SAE data.

>   See Configuring the Directory Location for SAE Data with the C-Web Interface

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.