> - Downloads
> - Configuring the SAE for a Cable Network Environment (C-Web Interface)
> - Related Topics
> - Configuring the SAE for a Cable Network Environment (SRC CLI)
> - Using the SAE in a PCMM Environment
> - Overview of a PCMM Environment

> # Configuring the SAE for a Cable Network Environment (C-Web Interface)

> The tasks to configure the SAE for a cable network environment are:

> 1. Configure the SAE to manage PCMM devices.

>    See Configuring the SAE to Manage PCMM Devices (C-Web Interface).

> 2. Configure the session store.
> 3. Set up SAE communities.

>    See Setting Up SAE Communities (C-Web Interface).

> 4. (Optional) Configure SAE properties for the Event Notification API.

>    See Configuring SAE Properties for the Event Notification API (C-Web Interface) (if you are using an external address manager).

> 5. (Optional) Configure record-keeping server peers for plug-ins.

>    See Configuring Record-Keeping Server Peers for Plug-Ins (C-Web Interface) (if you are using the RKS plug-in).

> 6. (Optional) Configure PCMM record-keeping server plug-ins.

>    See Configuring PCMM Record-Keeping Server Plug-Ins (C-Web Interface) (if you are using the SAE’s embedded policy server).

> In addition to configuring the SAE, you need to:

> 1. Configure the CMTS device in the directory (if you are using the SAE’s embedded policy server).

>    See Adding Objects for CMTS Devices (C-Web Interface) .

> 2. Configure the NIC (if you are using assigned IP subscribers).

>    See Using the NIC Resolver in PCMM Environments .

> 3. Enable the Common Open Policy Service (COPS) interface on the CMTS device. See the documentation for your CMTS device for information about how to do this.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.