[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring NTP Broadcast Mode on a C Series Controller (C-Web Interface)

To configure NTP to operate in broadcast mode:

1. Click Configure, expand System, and click NTP.

   The NTP pane appears.

2. In the Create new list, select Broadcast. Type an IP address or a hostname on one of the local networks or a multicast address assigned to NTP. Click OK.
3. Enter information as described in the Help text in the main pane, and click Apply.

   | Note: If the remote system has authentication enabled, specify an authentication key and value. The system transmits the specified authentication key when transmitting packets.

#### Related Topics

- NTP Support on C Series Controllers
- Configuring NTP on a C Series Controller

[Contents] [Prev] [Next] [Index] [Report an Error]