[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the SAE Community Manager

Use the following configuration statements to configure the SAE community manager that manages PCMM device communities:

`

shared sae configuration external-interface-features name CommunityManager {
  keepalive-interval keepalive-interval ;
  threads threads ;
  acquire-timeout acquire-timeout ;
  blackout-time blackout-time ;
}

`

To configure the community manager:

1. From configuration mode, access the configuration statements for the community manager. In this sample procedure, west_region is the name of the SAE group, and sae_mgr is the name of the community manager.
   `
   user@host# edit shared sae group west-region configuration external-interface-features sae_mgr CommunityManager
   `
2. Specify the interval between keepalive messages sent from the active SAE to the passive members of the community.
   `
   [edit shared sae group west-region configuration external-interface-features sae_mgr CommunityManager]
   user@host# set keepalive-interval keepalive-interval
   `
3. Specify the number of threads that are allocated to manage the community. You generally do not need to change this value.
   `
   [edit shared sae group west-region configuration external-interface-features sae_mgr CommunityManager]
   user@host# set threads threads
   `
4. Specify the amount of time an SAE waits for a remote member of the community when it is acquiring a distributed lock. You generally do not need to change this value.
   `
   [edit shared sae group west-region configuration external-interface-features sae_mgr CommunityManager]
   user@host# set acquire-timeout acquire-timeout
   `
5. Specify the amount of time that an active SAE must wait after it shuts down before it can try to become the active SAE of the community again.
   `
   [edit shared sae group west-region configuration external-interface-features sae_mgr CommunityManager]
   user@host# set blackout-time blackout-time
   `
6. (Optional) Verify the configuration of the SAE community manager.

       [edit shared sae group west-region configuration external-interface-features sae_mgr CommunityManager]
       user@host# show
       CommunityManager {
         keepalive-interval 30;
         threads 5;
         acquire-timeout 15;
         blackout-time 30;
       }

#### Related Topics

- Using the SAE in a PCMM Environment
- Configuring the SAE Community Manager with the C-Web Interface
- Setting Up SAE Communities (SRC CLI)
- Initially Configuring the SAE .

[Contents] [Prev] [Next] [Index] [Report an Error]