[Contents] [Prev] [Next] [Index] [Report an Error]

# Adding Objects for CMTS Devices (C-Web Interface)

To manage CMTS devices, the SAE creates and manages pseudointerfaces that it associates with a virtual router object. Each CMTS device in the SRC network must appear in the configuration as a router object, and it must be associated with a virtual router object called default. The router and virtual router are not actually configured on the CMTS device; the router and virtual router provide a way for the SAE to manage the CMTS device by using the SAE’s embedded policy server.

To add a router:

1. Click Configure, expand Shared, and then click Network.

   The Shared Network pane appears.

2. From the Create new list, select Device.
3. Type a name for the new device in the dialog box, and click OK.

   The Device pane appears.

4. From the Device Type list, select pccm.
5. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Creating Virtual Routers for the CMTS Device (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]