[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Next-Interface Actions (C-Web Interface)

Use this action to forward packets to a particular interface and/or a next-hop address. You can configure next-interface actions for JUNOS filters and JUNOSe policy rules. On JUNOSe routers, you can use this action for both ingress and egress parts of the interface.

To configure a next-interface action:

1. In the side pane, select a JUNOS filter or JUNOSe policy rule.
2. From the Create new list, select Next Interface. Type a name for the action, and click OK.
3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Next-Interface Actions (SRC CLI)
- Configuring Next-Hop Actions (C-Web Interface)
- Configuring Next-Rule Actions (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]