[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring SRC ACP to Manage the Backbone Network (C-Web Interface)

To configure SRC ACP to manage the backbone network:

1. Configure network interfaces in the directory.

   See Configuring Network Interfaces in the Directory .

2. (Optional) Configure an action congestion point.

   See Configuring Action Congestion Points.

3. Configure guaranteed bandwidths for services.
4. Assign network interfaces to services.

   See Configuring Congestion Points for Services

5. Create congestion points in the directory.

   See Configuring Congestion Points in the Directory

6. Assign interfaces to congestion points.

   See Assigning Interfaces to Congestion Points

#### Related Topics

- Configuring SRC ACP (C-Web Interface)
- Configuring SRC ACP to Manage the Edge Network (C-Web Interface)
- Configuring SRC ACP to Manage the Backbone Network
- Configuring Action Congestion Points

[Contents] [Prev] [Next] [Index] [Report an Error]