[Contents] [Prev] [Next] [Index] [Report an Error]

# Starting the SRC Client on a JUNOSe Router

JUNOSe routers use an SRC client to interact with the SAE. See JUNOSe Broadband Access Configuration Guide for complete information about configuring the SRC client on a JUNOSe router.

To start the SRC client:

1. Access the router CLI.
2. Access Global configuration mode.
   `
   host1# configure terminal
   `
3. Switch to the virtual router for which you want to create an SRC client.
   `
   host1(config)#virtual-router <vrName>
   `
4. Enable the SRC client.

   To enable COPS-PR mode:

   `
   host1:<vrName>(config)#sscc enable cops-pr
   `

   To enable COPS-XDR mode:

   `
   host1:<vrName>(config)#sscc enable
   `
5. Set the primary address from the configuration directory.
   `
   host1:<vrName>(config)#sscc primary address <ipAddress> port 3288
   `

#### Related Topics

- Stopping the SRC Client on a JUNOSe Router
- Accessing the Router CLI
- Specifying Router Initialization Scripts on the SAE with the CLI
- Viewing Statistics for All JUNOSe Device Drivers (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]