[Contents] [Prev] [Next] [Index] [Report an Error]

## Before You Configure Classify-Traffic Conditions

If you are configuring classifiers for policies:

- For PCMM policies, you can specify that the classifier will be used in a PCMM IO2 or IO3 network. By default, the software translates classify-traffic conditions into PCMM IO2 classifiers.
- For JUNOSe policies, you can specify that the SAE expand the classifier into multiple classifiers before it installs the policy on the router.

#### Related Topics

- Configuring Classify-Traffic Conditions
- Enabling Expansion of JUNOSe Classify-Traffic Conditions (SRC CLI)
- Specifying the PCMM Classifier Type (SRC CLI)
- Specifying Port Access for Traffic Classification (SRC CLI)
- Creating a Classify-Traffic Condition (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]