> - Downloads
> - Configuring the SAE to Manage JUNOS Routing Platforms (C-Web Interface)
> - Related Topics
> - Configuring the SAE to Manage JUNOS Routing Platforms
> - Configuring Secure Connections Between the SAE and JUNOS Routing Platforms
> - Configuring JUNOS Routing Platforms to Interact with the SAE
> - Setting Up the SAE to Periodically Check JUNOS Configuration (C-Web Interface)
> - Monitoring Interactions Between the SAE and JUNOS Routing Platforms

> # Configuring the SAE to Manage JUNOS Routing Platforms (C-Web Interface)

> A JUNOS routing platform interacts with the SAE by using a JUNOS software process called sdxd. When the sdxd process establishes a TCP/IP connection to the SAE, the SAE begins to manage the router. The JUNOS router driver configuration defines parameters related to the interactions between the SAE and the sdxd process.

> To configure the SAE to manage JUNOSe routers:

> 1. Click Configure, expand Shared>SAE>Configuration>Driver, and then click JUNOS.

>    The JUNOS pane appears.

> 2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.