> - Downloads
> - Configuring Subscriber IP Pools as IP Address Ranges
> - Related Topics
> - Configuring Subscriber IP Pools as IP Address Ranges (C-Web Interface)
> - Modifying the Subscriber Configuration
> - Configuring Subscriber IP Pools as IP Subnets
> - Specifying Connections to CMTS Devices

> # Configuring Subscriber IP Pools as IP Address Ranges

> To configure subscriber IP pools that are managed by the CMTS device as IP address ranges:

> 1. From configuration mode, access the configuration statement that configures the CMTS device to which the JPS can connect.
>    `
>    user@host# edit slot 0 jps cmts-registry cmts cmts-ip range-pool pool-index
>    `

>    Specify the IP address of the CMTS device and the address range pool index.

> 2. Specify the first IP address in the IP range for the pool of subscriber IP addresses that are managed by the CMTS device.
>    `
>    [edit slot 0 jps cmts-registry cmts cmts-ip range-pool pool-index]
>    user@host# set low low
>    `
> 3. Specify the last IP address in the IP range for the pool of subscriber IP addresses that are managed by the CMTS device.
>    `
>    [edit slot 0 jps cmts-registry cmts cmts-ip range-pool pool-index]
>    user@host# set high high
>    `
> 4. (Optional) Verify your configuration.

>        [edit slot 0 jps cmts-registry]
>        user@host# show

> #### Published: 2009-09-23

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.