> - Downloads
> - Configuring TLS on the SAE
> - Related Topics
> - Configuring the SAE to Use TLS
> - Configuring the SAE to Manage JUNOS Routing Platforms (C-Web Interface)
> - Monitoring Interactions Between the SAE and JUNOS Routing Platforms

> # Configuring TLS on the SAE

> To configure TLS on the SAE:

> 1. Click Configure, expand Shared>SAE>Configuration>Driver>JUNOS, and then click Security.

>    The Security pane appears.

> 2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.