[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Gigabit Ethernet Interfaces for IPv6 (SRC CLI)

You can configure the Gigabit Ethernet interfaces to use IPv4 or IPv6 to allow remote access to the C Series Controller. You can specify an IP address with mask or a broadcast address with mask for an interface.

Use the following configuration statement to configure Gigabit Ethernet interfaces to use IPv6 at the [edit] hierarchy level:

`

interfaces name unit unit-number family inet6 address address ;

`

To configure a Gigabit Ethernet interface to use IPv6:

1. From configuration mode, access the configuration statement that configures the interface.
   `
   [edit]
   user@host# edit interfaces name unit unit-number
   `

   where unit-number is a number that you can assign for a logical interface identifier.

   For example:

   `
   [edit]
   user@host# edit interfaces eth0
   `
2. Specify the unit, family, and IP address for the interface.
   `
   [edit interfaces eth0]
   user@host# set unit number family inet6 address address
   `

   For example:

   `
   [edit interfaces eth0]
   user@host# set unit 0 family inet6 address 2001:DB8:10AB:CD30::1/64
   `
3. Verify the interface configuration.

       [edit interfaces eth0]
       user@host# show
       unit 0 {
         family {
           inet6 {
             address 10AB:0:0:CD30::/20;
           }
         }
       }

#### Related Topics

- Configuring Gigabit Ethernet Interfaces for IPv6 (C-Web Interface)
- Configuring Gigabit Ethernet Interfaces for IPv4 (SRC CLI)
- Configuring Tunnel Interfaces (SRC CLI)
- Overview of External Interfaces on a C Series Controller

[Contents] [Prev] [Next] [Index] [Report an Error]