[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the SAE to Use TLS

To configure the SAE to accept TLS connections:

1. Click Configure, expand Shared>Network, and then click a JUNOS router.

   The Device pane appears.

2. Type a port number in the Beep Server Port box, and click Apply.

#### Related Topics

- Configuring the SAE to Manage JUNOS Routing Platforms (C-Web Interface)
- Configuring TLS on the SAE
- Configuring JUNOS Routing Platforms to Interact with the SAE
- Monitoring Interactions Between the SAE and JUNOS Routing Platforms

[Contents] [Prev] [Next] [Index] [Report an Error]