> - Downloads
> - Configuring Authentication (C-Web Interface)
> - Related Topics
> - Configuring Encryption (C-Web Interface)
> - Configuring Authentication
> - Configuring Access Control for SNMPv3 Users (C-Web Interface)
> - Defining Access Privileges for an SNMP Group (C-Web Interface)

> # Configuring Authentication (C-Web Interface)

> To configure the authentication type for SNMPv3 users:

> 1. Click Configure, and expand SNMP>V3>USM>Local Engine.
> 2. To configure MD5 authentication, from the side pane, expand the name of the user, and click Authentication MD5.
> 3. To configure SHA authentication, from the side pane, expand the name of the user, and click Authentication SHA.
> 4. Specify the authentication password as described in the Help text in the main pane, and then click Create.

>    The password must be at least eight characters.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.