[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring DOCSIS Actions (C-Web Interface)

You can configure Data over Cable Service Interface Specifications (DOCSIS) actions for PacketCable Multimedia Specification (PCMM) policy rules.

The types of DOCSIS actions that you can create are:

- Best effort
- Downstream
- Non-real-time polling service
- Real-time polling service
- Unsolicited grant service
- Unsolicited grant service with activity detection
- Parameter—This is a DOCSIS action with the service flow scheduling type set to a trafficProfileType parameter. You must enter a trafficProfileType parameter that has been created and committed.

To configure a DOCSIS action:

1. In the side pane, select a PCMM policy rule.
2. From the Create new list, select the type of DOCSIS action that you want to create. Type a name for the action, and click OK.
3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Delivering QoS Services in a Cable Environment
- Configuring DOCSIS Actions (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]