> - Downloads
> - Specifying Port Access for Traffic Classification (C-Web Interface)
> - Related Topics
> - Before You Configure Classify-Traffic Conditions
> - Configuring Classify-Traffic Conditions (C-Web Interface)
> - Specifying Port Access for Traffic Classification (SRC CLI)
> - Specifying the PCMM Classifier Type (C-Web Interface)

> # Specifying Port Access for Traffic Classification (C-Web Interface)

> You can specify a range of port numbers greater than or less than a specific value in a traffic classifier is different from the way you define a range in the configuration on JUNOSe routers.

> In the C-Web interface, you specify ranges by setting values in the Port Operation boxes.

> To specify a range of port numbers greater or less than a specified value, you can:

> - Define the full set of port numbers in the range to be allowed.
> - Define the full set of port numbers in the range not allowed.

> To configure port numbers greater than a defined value by specifying which values are allowed:

> 1. From the Port Operation list, select eq.
> 2. In the From Port box, enter the range of ports allowed.

>    For example, to specify access to all port numbers greater than 10, specify 11..65535.

> To configure port numbers greater than a defined value by specifying which values are not allowed:

> 1. From the Port Operation list, select neq.
> 2. In the From Port box, enter the range of ports not allowed.

>    For example, to specify access to all port numbers greater than 10, specify 1..9.

> To configure port numbers less than a defined value by specifying which values are allowed:

> 1. From the Port Operation list, select eq.
> 2. In the From Port box, enter the range of ports.

>    For example, to specify access to all port numbers less than 10, specify 1..9.

> To configure port numbers less than a defined value by specifying which values are not allowed:

> 1. From the Port Operation list, select neq.
> 2. In the From Port box, enter the range of ports.

>    For example, to specify access to all port numbers less than 10, specify 11..65535.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.