[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the SAE to Use TLS

To configure the SAE to accept TLS connections, enter a port number with the set beep-server-port command in the JUNOS router driver configuration.

See Configuring the SAE to Manage JUNOS Routing Platforms .

#### Related Topics

- Configuring the SAE to Use TLS
- Configuring TLS on the SAE
- Configuring JUNOS Routing Platforms to Interact with the SAE
- Monitoring Interactions Between the SAE and JUNOS Routing Platforms

[Contents] [Prev] [Next] [Index] [Report an Error]