[Contents] [Prev] [Next] [Index] [Report an Error]

## Use of Multiple SRC ACPs

An SRC ACP can support one or more SAEs. Similarly, multiple SRC ACPs can support one SAE; for example, if an SAE is managing multiple VRs, you may have an SRC ACP for each VR. However, only one SRC ACP can manage a particular congestion point.

#### Related Topics

- Overview of SRC ACP
- Allocating Bandwidth to Applications Not Controlled by SRC ACP
- Interactions Between SRC ACP and Other Components
- Configuring the SAE for SRC ACP
- Configuring SRC ACP
- Configuring SRC ACP Properties

[Contents] [Prev] [Next] [Index] [Report an Error]