[Contents] [Prev] [Next] [Index] [Report an Error]

# Removing and Installing a Power Supply Module

| Note: If your system is powered on, see the SRC PE CLI User Guide, Chapter 5, Using the SRC CLI Operational Commands to Monitor the SRC Software for commands to run before performing these steps.

To remove a power supply module:

1. Unplug the power cord.
2. Slide the locking tab (ejector button) to the left to release the module. See Figure 14 and Figure 15.
3. Hold the tab to the left, and using the handle, slowly pull the power supply module out.

To install a power supply module:

1. Hold the locking tab (ejector button) to the left, and slowly slide the module into the chassis until it clicks into place.
2. Insert the power cord into the AC power IEC receptacle.

Figure 14: C2000 Power Supply

Figure 15: C4000 Power Supply

[Contents] [Prev] [Next] [Index] [Report an Error]