> - Downloads
> - Configuring SRC ACP Properties (C-Web Interface)
> - Related Topics
> - Configuring SRC ACP Properties
> - Configuring Local Properties for SRC ACP
> - Configuring SRC ACP
> - Configuring SRC ACP to Manage the Edge Network
> - Overview of SRC ACP

> # Configuring SRC ACP Properties (C-Web Interface)

> - Configuring Logging Destinations for SRC ACP
> - Configuring SRC ACP Operation
> - Configuring CORBA Interfaces
> - Configuring SRC ACP Redundancy
> - Configuring Connections to the Subscribers’ Directory
> - Configuring Connections to the Services’ Directory
> - Configuring SRC ACP Scripts and Classification

> ## Configuring Logging Destinations for SRC ACP

> SRC ACP groups contain default file logging configurations. You can modify an existing configuration or create a new one.

> To modify logging destinations that store log messages in a file:

> 1. Click Configure>Shared>ACP, expand the group for which you want to configure logging and expand Configuration.

>    Several Logger:file configurations appear.

> 2. In the Create new list, select Logger.
> 3. Type a name for the new logger in the dialog box, and click OK.

>    The logger appears in the side pane.

> 4. Select the configuration that you want to modify, enter information as described in the Help text in the main pane, and click Apply.

> To create logging destinations to store log messages in a file:

> 1. Click Configure>Shared>ACP, and expand the group for which you want to configure logging destinations and expand Configuration.
> 2. From the Create new list, select Logger.
> 3. Type a name for the new logging configuration, and click OK.

>    The logger appears in the side pane.

> 4. Expand the new logging configuration, select File, and enter information as described in the Help text in the main pane, and click Apply.

> You can configure logging destinations to send log messages to the system logging facility. SRC ACP groups contain default system logging configurations. You can modify an existing configuration or create a new one.

> To modify an existing system logging configuration:

> 1. Click Configure>Shared>ACP, expand the group for which you want to modify an existing configuration, and expand Configuration.

>    Several Logger:syslog configurations appear.

> 2. Select the configuration that you want to modify, enter information as described in the Help text in the main pane, and click Apply.

> To create a configuration that causes logging destinations to send log messages to the system logging facility:

> 1. Click Configure>Shared>ACP, and expand the group for which you want to modify an existing configuration.
> 2. In the Create new list, select Logger. Type a name for the new logging configuration, and click OK.

>    The logger appears in the side pane.

> 3. Expand the new logging configuration, select Syslog, and enter information as described in the Help text in the main pane, and click Apply.

> ## Configuring SRC ACP Operation

> To configure SRC ACP operation:

> 1. Click Configure>Shared>ACP, expand the group for which you want to modify an existing configuration, and expand Configuration.
> 2. Click ACP Options, enter information as described in the Help text in the main pane, and click Create.
> 3. In the Remote Update Database Index Keys box, specify the values to look for in the configuration data. Specifying index keys can improve performance by filtering the data.

>    The value is a list of attributes, separated by commas. An attribute is one of the following text strings:

>    - accountingId—Value of directory attribute accountingUserId.
>    - dhcpPacket—Content of the DHCP discover request.
>    - hostname— Name of the host on which the SAE is installed.
>    - ifIndex—SNMP index of the interface. This attribute is not supported on JUNOS routing platforms.
>    - ifRadiusClass—RADIUS class attribute on the JUNOSe interface. This attribute is not supported on JUNOS routing platforms.
>    - ifSessionId—Identifier for RADIUS accounting on the JUNOSe interface. This attribute is not supported on JUNOS routing platforms.
>    - interfaceAlias—Alias of the interface; that is, the IP description in the interface configuration.
>    - interfaceDescr—SNMP description of the interface.
>    - interfaceName—Name of the interface.
>    - loginName—Subscriber's login name.
>    - nasInetAddress—IP address of the router; using a byte array instead of an integer.
>    - nasPort—NAS port used by the router to identify the interface to RADIUS.
>    - portId—Identifier of VLAN or virtual circuit. For a virtual circuit, use the format <VPI>/<VCI>. This attribute is not supported on JUNOS routing platforms.
>      - <VPI>—Virtual path identifier
>      - <VCI>—Virtual connection identifier
>    - primaryUserName—PPP login name or the public DHCP username. This attribute is not supported on JUNOS routing platforms.
>    - routerName—Name of the virtual router in the format <virtualRouter>@<router>.
>      - <virtualRouter>—Virtual router name
>      - <router>—Router name
>    - routerType—Type of router driver.
>    - userInetAddress—IP address of the subscriber that uses a byte array instead of an integer.
>    - userMacAddress—MAC address of the DHCP subscriber. This attribute is not supported on JUNOS routing platforms.
>    - userRadiusClass—RADIUS class attribute of the subscriber session for a service. This attribute can occur multiple times and can be returned by an authorization plug-in.
>    - userType—Type of subscriber.
> 4. In the Interface Tracking Filter box, specify the interface tracking events that the SRC ACP ignores.

>    The value is filter strings in the format of a list of <attribute>=<value> pairs. The filter strings can be contained within query operations.

>    - <attribute>—Name of an attribute for an interface tracking event.
>    - <value>—Filtering string of the following types:
>      - *—Any value
>      - Explicit string—Any value matching the specified string (not case-sensitive)
>      - String containing an asterisk—Any value containing the specified string (not case-sensitive)
>    - To perform query operations on filter strings, you can use the following values in your filter strings:
>      - ()—Match no objects.
>      - (*)—Match all objects.
>      - (&<filter><filter>...)—Performs logical AND operation on filter strings; true if all filter strings match.
>      - (|<filter><filter>...)—Performs logical OR operation on filter strings; true if at least one filter string matches.
>      - (!<filter>)—Performs logical NOT operation on filter string; true if the filter string does not match.

> ## Configuring CORBA Interfaces

> To configure CORBA interfaces:

> 1. Click Configure>Shared>ACP > Configuration , and then click CORBA.

>    The CORBA pane appears.

> 2. Click Create, enter information as described in the Help text in the main pane, and click Apply.

> ## Configuring SRC ACP Redundancy

> To configure SRC ACP redundancy and state synchronization with the SAE:

> 1. Click Configure>Shared>ACP > Redundancy.

>    The Redundancy pane appears.

> 2. Enter information as described in the Help text in the main pane, and click Apply.

> ## Configuring Connections to the Subscribers’ Directory

> To configure how SRC ACP connects to the directory that stores subscriber information:

> 1. Click Configure>Shared>ACP > LDAP, and expand Subscriber Data.

>    The Subscriber Data pane appears.

> 2. Enter information as described in the Help text in the main pane, and click Apply.

> ## Configuring Connections to the Services’ Directory

> To configure how SRC ACP connects to the directory that stores service information:

> 1. Click Configure>Shared>ACP > LDAP, and expand Service Data.

>    The Service Data pane appears.

> 2. Enter information as described in the Help text in the main pane, and click Apply.

> ## Configuring SRC ACP Scripts and Classification

> To configure SRC ACP scripts and classification:

> 1. Click Configure>Shared>ACP > Configuration and then expand Scripts and Classification.

>    The Scripts and Classification pane appears.

> 2. Click Create, enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.