> - Downloads
> - Specifying Connections to CMTS Devices (C-Web Interface)

> # Specifying Connections to CMTS Devices (C-Web Interface)

> To configure the policy server–to–CMTS interface (PKT-MM2) so that the policy server can communicate with CMTS devices:

> 1. Click Configure, expand Slot>Slot: 0>JPS, and then click CMTS Interface.

>    The CMTS Interface pane appears.

> 2. Enter the information in the main pane as described in the Help text, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.