[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring FlowSpec Actions (C-Web Interface)

A FlowSpec is made up of two parts, a traffic specification (TSpec) and a service request specification (RSpec). The TSpec describes the traffic requirements for the flow, and the RSpec specifies resource requirements for the desired service. You can configure FlowSpec actions for PCMM policy rules.

To configure a FlowSpec action:

1. In the side pane, select a PCMM policy rule.
2. From the Create new list, select Flow Spec. Type a name for the action, and click OK.
3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Delivering QoS Services in a Cable Environment
- Configuring FlowSpec Actions (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]