> - Downloads
> - Configuring CMTS-Specific RKS Plug-Ins (C-Web Interface)
> - Related Topics
> - Configuring CMTS-Specific RKS Plug-Ins (SRC CLI)
> - Adding Objects for CMTS Devices (SRC CLI)
> - Creating Virtual Routers for the CMTS Device (SRC CLI)

> # Configuring CMTS-Specific RKS Plug-Ins (C-Web Interface)

> You can configure an RKS plug-in for specific CMTS devices. When there are events for the CMTS device, the SAE sends the events to the specified plug-in.

> To configure a CMTS-specific RKS plug-in:

> 1. Click Configure, expand Shared>SAE,>Configuration>Driver, and then click PCCM.
> 1. Click Configure, expand Shared>SAE, and then expand the SAE group for which you want to create CMTS-specific RKS plug-ins.
> 2. In the side pane, expand Configuration>Drivers, and then click PCCM.

>    The PCMM pane appears.

> 3. From the Create new list, select CMTS Specific RKS Plug-Ins.
> 4. Type a name for the new plug-in in the dialog box, and click OK.
> 5. In the side pane, click the new plug-in.
> 6. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.