[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring SAE Properties for the Event Notification API (SRC CLI)

Use the following configuration statements to configure properties for the Event Notification API:

`

shared sae configuration external-interface-features name EventAPI {
  retry-time retry-time ;
  retry-limit retry-limit ;
  threads threads ;
}

`

To configure properties for the Event Notification API:

1. From configuration mode, access the configuration statements for the Event Notification API. In this sample procedure, west-region is the name of the SAE group, and event_api is the name of the Event API configuration.
   `
   user@host# edit shared sae group west-region configuration external-interface-features event_api EventAPI
   `
2. Specify the amount of time between attempts to send events that could not be delivered.
   `
   [edit shared sae group west-region configuration external-interface-features event_api EventAPI]
   user@host# set retry-time retry-time
   `
3. Specify the number of times an event fails to be delivered before the event is discarded.
   `
   [edit shared sae group west-region configuration external-interface-features event_api EventAPII]
   user@host# set retry-limit retry-limit
   `
4. Specify the number of threads allocated to process events.
   `
   [edit shared sae group west-region configuration external-interface-features event_api EventAPI]
   user@host# set threads threads
   `
5. (Optional) Verify the configuration of the Event Notification API properties.

       [edit shared sae group west-region configuration external-interface-features event_api EventAPI]
       user@host# show
       EventAPI {
         retry-time 300;
         retry-limit 5;
         threads 5;
       }

#### Related Topics

- Using the SAE in a PCMM Environment
- Configuring SAE Properties for the Event Notification API (C-Web Interface)
- Initially Configuring the SAE
- Configuring the SAE to Manage PCMM Devices (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]