> - Downloads
> - Before You Configure Classify-Traffic Conditions
> - Related Topics
> - Configuring Classify-Traffic Conditions
> - Enabling Expansion of JUNOSe Classify-Traffic Conditions (SRC CLI)
> - Specifying the PCMM Classifier Type (SRC CLI)
> - Specifying Port Access for Traffic Classification (SRC CLI)
> - Creating a Classify-Traffic Condition (SRC CLI)

> ## Before You Configure Classify-Traffic Conditions

> If you are configuring classifiers for policies:

> - For PCMM policies, you can specify that the classifier will be used in a PCMM IO2 or IO3 network. By default, the software translates classify-traffic conditions into PCMM IO2 classifiers.
> - For JUNOSe policies, you can specify that the SAE expand the classifier into multiple classifiers before it installs the policy on the router.

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.