[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring RADIUS and TACACS+ Authentication on a C Series Controller

The SRC software always performs password authentication on a C Series Controller. You can configure RADIUS or TACACS+ (or both) authentication to complement password authentication. In this case, the software performs RADIUS or TACACS+ (or both) authentication before password authentication.

To configure RADIUS and TACACS+ authentication for users who access a C Series Controller:

1. Configure the connection to the RADIUS or TACACS+ server.

   See Configuring RADIUS Authentication (SRC CLI).

2. Configure the authentication order.

   See A C Series Controller as a RADIUS Client and TACACS+ Client .

3. Configure template accounts.
4. (Optional) Configure individual user profiles.

   See Overview of SRC User Accounts.

#### Related Topics

- Configuring RADIUS and TACACS+ Authentication on a C Series Controller (C-Web Interface)
- Configuring TACACS+ Authentication (C-Web Interface)
- Removing an SRC Authentication Method from the Authentication Order
- Example: Configuring SRC Authentication

[Contents] [Prev] [Next] [Index] [Report an Error]