[Contents] [Prev] [Next] [Index] [Report an Error]

# Setting Up SAE Communities (SRC CLI)

You can configure the following for SAE communities:

- Define the members of an SAE community by adding the IP addresses of SAEs in the community to the virtual router object of the network device in the directory.

  See Creating Virtual Routers for the CMTS Device (SRC CLI) .

- Configure parameters for the SAE community manager.

  See Configuring the SAE Community Manager .

- Specify the name of the community manager with the set sae-community-manager option in the PCMM driver configuration.

  See Configuring the SAE to Manage PCMM Devices (SRC CLI).

- If there is a firewall in the network, configure the firewall to allow SAE messages through.

#### Related Topics

- Using the SAE in a PCMM Environment
- Setting Up SAE Communities (C-Web Interface)
- Initially Configuring the SAE
- Configuring SAE Properties for the Event Notification API (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]