> - Downloads
> - Interface Classification Conditions

> ## Interface Classification Conditions

> Use the fields in this section to define interface classification conditions.

> broadcastAddr

> - Interface broadcast address.
> - Value—Valid broadcast address format
> - Example—broadcastAddr.hostAddress=“ 255.255.255.255”

> ifAlias

> - Description of an interface.
> - Value—Interface description that is configured on the router. For JUNOSe routers, it is the description configured with the interface description command.
> - Example—ifAlias=“ 1st pppoe int”

> ifDesc

> - Alternate name of the interface that is used by SNMP. This name is a system-generated name.
> - Value
>   - On a JUNOSe router, the format of the description is
>     `
>     ip<slot>/<port>.<subinterface>
>     `
>   - On the JUNOS routing platform, ifDesc is the same as interfaceName.
> - Example—ifDesc=“ IP3/1.1”

> interfaceName

> - Name of the interface.
> - Value
>   - Name of the interface in your router CLI syntax
>   - FORWARDING_INTERFACE for routing instance (used by traffic mirroring)
> - Example—For JUNOSe routers: interfaceName=“ fastethernet6/0.1”

> For JUNOS routing platforms: interfaceName=“ fe-0/1/0.0”

> For forwarding interface: interfaceName=“ FORWARDING_INTERFACE”

> ipAddress

> - Interface IP address.
> - Value—Valid IPv4 IP address format
> - Example—ipAddress=“ 10.10.30.1”

> ipMask

> - Interface network mask.
> - Value—Valid IPv4 IP network mask format
> - Example—ipMask=“ 255.255.255.255”

> mtu

> - Maximum transfer unit configured on the interface.
> - Value—32-integer value
> - Example—mtu=“ 1492”

> nasPortId

> - Port identifier of an interface.
> - Value—Includes interface name and additional layer 2 information
> - Example—nasPortId=“ fastEthernet 3/1” (There is a space between fastEthernet and slot number 3/1 in the nasPortId.)

> pppLoginName

> - Login name for PPP subscribers.
> - Value—Login name in the format username@domain
> - Example—pppLoginName=“ pebbles@virneo.net”

> radiusClass

> - RADIUS class attribute.
> - Value—RADIUS class name
> - Example—radiusClass=“ Premium”

> serviceBundle

> - Content of the vendor-specific RADIUS attribute for the service bundle.
> - Value—Name of a service bundle

> userIpAddress

> - Subscriber IP address (PPP only).
> - Value—valid IPv4 address
> - Example—userIpAddress=“ 192.168.30.15”

> virtualRouterName

> - Name of the virtual router or routing instance.
> - Value—For JUNOSe routers: name of the virtual router in the format vrname@hostname

>   For JUNOS routing platforms: name of the routing instance

> - Example—virtualRouterName=“ default@erx5”

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.