> - Downloads
> - Configuring RADIUS and TACACS+ Authentication on a C Series Controller (C-Web Interface)
> - Related Topics
> - Configuring RADIUS and TACACS+ Authentication on a C Series Controller
> - Configuring Authentication Order
> - Removing an Authentication Method from the Authentication Order

> # Configuring RADIUS and TACACS+ Authentication on a C Series Controller (C-Web Interface)

> The SRC software always performs password authentication on a C Series Controller. You can configure RADIUS and/ or TACACS+ authentication to complement password authentication. In this case, the software performs RADIUS and/or TACACS+ authentication before password authentication.

> To configure RADIUS and TACACS+ authentication for users who access a C Series Controller:

> 1. Configure the connection to the RADIUS or TACACS+ server.

>    See Configuring RADIUS Authentication (C-Web Interface).

>    See Configuring TACACS+ Authentication (C-Web Interface).

> 2. Configure the authentication order.
> 3. Configure template accounts.

>    See Using Remote Template Accounts and Configuring a Local User Template.

> 4. (Optional) Configure individual user profiles.

>    See Overview of SRC User Accounts.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.