> - Downloads
> - Configuring the Directory Location for SAE Data with the C-Web Interface
> - Related Topics
> - Initially Configuring the SAE with the C-Web Interface
> - Configuring Local Properties for the SAE with the C-Web Interface
> - Configuring the RADIUS Local IP Address and NAS ID with the C-Web Interface

> # Configuring the Directory Location for SAE Data with the C-Web Interface

> You can configure the locations for dynamic and static configuration data in the directory.

> To configure the directory location for configuration data:

> 1. Click Configure, and expand Slot.
> 2. Expand the slot for which you want to configure SAE, expand SAE, and then click Initial.

>    The Initial pane appears.

> 3. Enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.