[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Access Control for the VACM (C-Web Interface)

To configure the access control for the view-based access control model (VACM):

1. Map an SNMPv1 or SNMPv2c community name to a security name.

   See Associating Security Names with a Community (C-Web Interface).

2. Define a named view.

   See Defining Named Views (C-Web Interface).

3. Map from a group of users or communities to a view.

   See Defining Access Privileges for an SNMP Group (C-Web Interface).

4. Map a security name into a named group.

   See Assigning Security Names to Groups (C-Web Interface).

#### Related Topics

- Configuring Access Control for the VACM
- Configuring Access Control for Communities (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]