[Contents] [Prev] [Next] [Index] [Report an Error]

## Configuration Statements for NTP on C Series Controllers

Use the following configuration statements to configure NTP on a C Series Controller at the [edit] hierarchy level.

`

system ntp {
  boot-server boot-server;
  broadcast-client;
  trusted-key [trusted-key...];
}
system ntp authentication-key key-number {
  value value;
}
system ntp broadcast address {
  key key ;
  ttl ttl ;
  version version ;
}
system ntp multicast-client {
  address;
}
system ntp peer address {
  key key;
  version version;
  prefer;
}
system ntp server address {
  key key;
  version version;
  prefer;
}

`

#### Related Topics

- SRC PE CLI Command Reference
- Configuring NTP on a C Series Controller
- NTP Support on C Series Controllers

[Contents] [Prev] [Next] [Index] [Report an Error]