[Contents] [Prev] [Next] [Index] [Report an Error]

# Specifying the PCMM Classifier Type (C-Web Interface)

To specify whether or not the SAE sends to the router classifiers that comply with PCMM I03:

1. Select Configure, expand Shared>SAE>Configuration>Driver, and select pcmm.
2. Check or clear the Disable PCMM I03 Policy box, and click Apply.

#### Related Topics

- Before You Configure Classify-Traffic Conditions
- Delivering QoS Services in a Cable Environment
- Configuring Classify-Traffic Conditions (C-Web Interface)
- Specifying the PCMM Classifier Type (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]