[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Information About Edge Congestion Points by Subscriber Session (C-Web Interface)

#### Purpose

View information about edge congestion points by subscriber session.

#### Action

To view information about edge congestion points:

1. Click ACP>Edge>Congestion Point>Subscriber Session ID.

   The Edge/Congestion Point/Subscriber Session ID pane appears.

2. In the Session ID box, enter a full or partial session ID name to display information about one or more specific sessions, or leave the box empty to display information about all sessions.
3. In the Slot box, enter the number of the slot for which you want to display congestion point information.
4. Select an output style from the Style list.
5. In the Virtual Router Name box, enter a virtual router name to display information about a specific virtual router, or leave the box empty to display information about all virtual routers.
6. Click OK.

   The Edge/Congestion Point/Subscriber Session ID pane displays a list of congestion points.

#### Related Topics

- Configuring SRC ACP to Manage the Edge Network (C-Web Interface)
- Viewing Information About Edge Congestion Points by Subscriber Session (C-Web Interface)
- Viewing Information About Edge Congestion Points by DN (C-Web Interface)
- Viewing Information About Subscriber Sessions in the Edge Network (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]