[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the JPS (C-Web Interface)

You can modify the JPS configuration, which includes configuring the logging destinations and connections to the JPS interfaces. Any configuration changes will be applied within 15 seconds.

You can configure the subscriber, which maps a subscriber address to the CMTS address.

The tasks to configure the JPS for a cable network environment are:

1. Modifying the JPS Configuration (C-Web Interface)
2. Modifying the Subscriber Configuration (C-Web Interface)

In addition to configuring the JPS, you might need to perform these tasks:

1. Configuring the SAE to Interact with the JPS (C-Web Interface)
2. Using the NIC Resolver in PCMM Environments .

#### Related Topics

- Configuring the JPS
- Starting the JPS (C-Web Interface)
- Displaying JPS Status (C-Web Interface)
- For information about monitoring the JPS with the C-Web interface, see the SRC PE Solutions Guide
- Overview of the JPS

[Contents] [Prev] [Next] [Index] [Report an Error]