[Contents] [Prev] [Next] [Index] [Report an Error]

# C4000 Model Specifications

Table 6: C4000 Model Specifications

Category | Specification
--- | ---
Weight | 48 lb (22 kg)
Dimensions | 3.5 (H) x 16.7 (W) x 24 (D) inches 8.89 (H) x 42.42 (W) x 60.96 (D) cm
Environmental Requirements |
Temperature | Operating: 50° to 104° F (10° to 40° C) Storage: –40° to 158° F (–40° ˚ to 70° C)
Relative humidity | Operating: 8% to 90% (noncondensing) Storage: 5% to 95% (noncondensing)
Ambient storage temperature | –40° ˚ to 158° F (–40° ˚ to 70° C), 95% relative humidity
Ambient storage humidity | 5% to 95% (noncondensing)
Heat Dissipation | 700 W, 2389 BTU/hour maximum
AC Input |
Power required | 90-264 VAC, 47–63 Hz
Power | 700 W
Efficiency | 80% minimum at full load
Space Requirements | 3 feet (90 cm) behind system or rack. Do not block air vents on or back of the system.
Airflow | Air intake occurs in the front of the system. Air is exhausted out of the rear of the system.
Safety Agency Certification | CAN/CSA-C22.2 No. 60950-1-03 EN 60950-1:2001+A11 EN 60825-1:1994+A1+A2 Low Voltage Directive 73/23/EEC UL 60950-1:2003
Electromagnetic Emissions Agency Certification | AZ/NZS CISPR 22:2002 EMC Directive (89/336/EEC) EN 55022:1998+A1 (2000)+A2(2003) Class A EN 55024: 1998+A1: 2001+A2: 2003 EN 61000-3-2:2001 EN 61000-3-3:1995 FCC Part 15 Subpart B VCCI (Voluntary Control Council for Interference by Information Technology Equipment)

[Contents] [Prev] [Next] [Index] [Report an Error]