> - Downloads
> - Configuring a NIC Proxy (C-Web Interface)
> - Related Topics
> - Before You Configure a NIC Proxy
> - Changing NIC Configurations (SRC CLI)
> - Configuring NIC Test Data (C-Web Interface)
> - Examples: Key Values for NIC Bindings
> - Overview of NIC Proxy Configuration

> # Configuring a NIC Proxy (C-Web Interface)

> To have an application communicate with the NIC, you configure the type of resolution used by a NIC proxy.

> To configure resolution information for a NIC proxy.

> 1. Click Configure, expand Shared>SAE, and then click Configuration.

>    The Configuration pane appears.

> 2. From the Create new list, select NIC Proxy Configuration. Type a name for the new NIC proxy in the dialog box, and click OK.

>    The new NIC proxy configuration appears in the side pane.

> 3. Expand the NIC proxy configuration.
> 4. To configure resolution information, in the side pane click Resolution.

>    The Resolution pane appears.

> 5. Click Create, enter information as described in the Help text, and click Apply.
> 6. To optimize resolution performance, in the side pane click Cache.

>    The Cache pane appears.

>    The cache options are available at the Advanced and Expert editing levels.

> 7. Click Create, enter information as described in the Help text, and click Apply.
> 8. To keep the NIC highly available, configure NIC host selection, and define how the NIC proxy handles NIC hosts to which it cannot connect.

>    The NIC Host Selection options are available at the Advanced and Expert editing levels.

>    1. In the side pane, click NIC Host Selection.

>       The NIC Host Selection pane appears.

>    2. Click Create, enter information as described in the Help text, and then click Apply.
>    3. Expand NIC Host Selection, and click Blacklisting.

>       The Blacklisting pane appears.

>    4. Click Create, enter information as described in the Help text, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.